{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":3,"rows_kept":3,"flags":["formulas_cached_only"]}
[null,"アクティブ時","スリープ時"]
["差込み検出","あり\nCDET端子\n High→Low","なし"]
["抜け検出","あり\nMC_IREQ (or MC_HOTSW)端子\n Low→High\n（ワンセグ等MC_IREQがリセット時\nHighの場合はROM-IDポーリング）","なし\n（レジューム後の検出で再ロード。\nNANDブートの場合PM_GoSleepMode\n内で強制無効化）"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}