{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":10,"n_cols":15,"rows_kept":10,"flags":["formulas_cached_only"]}
[null,"用途","用途詳細","配布先","HW種類","ボンディ\nング・オ\nプション","メニューUI","デバッガ対応","ランチャー基本機能\n（※２）","DSカードでTWLアプリブート","DSカードでDSアプリブート","無線AP設定","プロフィール入力","スケ\nジュール","備考"]
["A","DSモード\n検証","DSモードでの\n互換性検証","NEC, NOA, \nNOE, \nマリクラ","X4,\n量試品",10,"×","dc","dc","○","○","AP設定\nアプリ\n（※１）","ショートカット起動で本体設定を直接起動できるのがbetter。\n次策は、設定アプリでNAND,NORに書き込む","3月末\n（優先度やや低い）","Dと同じ?\nBO=00もミニ量試組立て時（4/7）に必要"]
["B","社内開発","ソフト開発／\nSDK開発","社内各部署、BroadOn","X4","01, 10","○","○","○","dc","dc","AP設定\nアプリ\n（※１）","メニューUIから","3月末"]
["C","社外ドライバ\n開発","無線ドライバ／\nブラウザコンポー\nネント開発も？","Atheros, Opera, Sharp","X4",10,"×","○","dc","dc","dc","AP設定\nアプリ\n（※１）","デバッガ＋\n設定アプリから","3月末"]
["D","社外検証","チップメーカー\nでの評価／無線\nAP接続テスト","TI, \nNEC, NOA, NOE, etc","X4",10,"×","dc","dc","○","dc","AP設定\nアプリ\n（※１）","DSカードTWLブート＋\n設定アプリから","3月末","Aと同じ?"]
["E","社内検証","ソフトのマリクラ\nデバッグ／無線\nAP接続テスト","社内各部署、\nマリクラ","量試品",10,"○","dc","dc","○","dc","AP設定\nアプリ\n（※１）","DSカードTWLブート＋\n設定アプリから","3月末","BO=00もミニ量試組立て時（4/7）に必要"]
[]
[{"$nulls":4},"○必須",null,"※１：TWLのNOR領域に、AP設定を書き込むアプリ"]
[{"$nulls":4},"×禁止",null,"※２：NANDインポート／アプリジャンプ等"]
[{"$nulls":4},"dcどっちでも可"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}