{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":38,"n_cols":5,"rows_kept":38,"merged":[[1,1,1,2],[11,1,11,2],[21,1,21,2],[29,2,29,4],[30,2,30,4],[33,1,34,1],[33,2,34,4],[35,1,36,1],[35,2,36,4],[37,1,38,1],[37,2,38,4]],"flags":["formulas_cached_only"]}
["デバッガ"]
[{"$nulls":3},"カードID d30=0(NTR)","カードID d30=1(TWL)"]
[null,"カード","DSアプリ","DSカード読み","DSカード読み"]
[null,null,"TWL-LTDアプリ","DSカード読み","TWLカード読み"]
[null,null,"TWL-HYBアプリ","DSカード読み","TWLカード読み"]
[null,"NAND","DSアプリ","DSカード読み","DSカード読み　※１"]
[null,null,"TWL-LTDアプリ","DSカード読み","DSカード読み　※１"]
[null,null,"TWL-HYBアプリ","DSカード読み","DSカード読み　※１"]
[]
[]
["開発用TWL本体"]
[{"$nulls":3},"DSカード","TWLカード"]
[null,"カード","DSアプリ","DSカード読み","DSカード読み"]
[null,null,"TWL-LTDアプリ","DSカード読み　※２","TWLカード読み"]
[null,null,"TWL-HYBアプリ","DSカード読み　※２","TWLカード読み"]
[null,"NAND　※３","DSアプリ","DSカード読み","DSカード読み　※１"]
[null,null,"TWL-LTDアプリ","DSカード読み　※２","DSカード読み　※１"]
[null,null,"TWL-HYBアプリ","DSカード読み　※２","DSカード読み　※１"]
[]
[]
["製品用TWL本体"]
[{"$nulls":3},"DSカード","TWLカード"]
[null,"カード","DSアプリ","DSカード読み","DSカード読み"]
[null,null,"TWL-LTDアプリ","不正カード判定","TWLカード読み"]
[null,null,"TWL-HYBアプリ","不正カード判定","TWLカード読み"]
[null,"NAND　※３","DSアプリ","DSカード読み","DSカード読み　※１"]
[null,null,"TWL-LTDアプリ","不正カード判定","DSカード読み　※１"]
[null,null,"TWL-HYBアプリ","不正カード判定","DSカード読み　※１"]
[]
[null,"DSカード読み","Normalモード → Secureモード → Gameモード"]
[null,"TWLカード読み","Noramlモード → Secureモード → スロット電源OFF → スロット電源ON → Normalモード → Secure2モード → Game2モード"]
[]
[]
[null," ※１","TWLカードだが境界値設定が0なのでメモリマップはNTRと同じになり、GameモードでSecure2領域 ,Game2領域が読める。"]
[]
[null," ※２","赤箱・ギャングライタでTWLカード書き込みに対応するまで(2008.7月下旬予定)は、TWLアプリ - DSカードの組み合わせはDSカード読み対応する。書き込みソフトが出来たら読み込めないようにする。"]
[]
[null," ※３","カードは読むがアプリ起動はしない。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}