{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["デバッガ","実機"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"デバッガ","index":0,"n_rows":104,"n_cols":22,"rows_kept":104,"flags":["formulas_cached_only"]}
[]
[null,"デバッガ確認"]
[]
[]
[null,"アプリブート確認",null,"確認用SRL","カード\nブート"]
[null,null,"NTRアプリ",null,"○"]
[null,null,"TWL-HYBアプリ　TWLモード",null,"○"]
[null,null,"TWL-HYBアプリ　NTRモード",null,"○"]
[null,null,"TWL-LTDアプリ",null,"○"]
[]
[null,"アプリロード範囲確認",null,"確認用SRL","確認"]
[null,null,"NTRアプリ"]
[null,null,"TWLアプリ"]
[]
[null,"アプリ再配置確認",null,"確認用SRL","確認"]
[null,null,"NTRアプリ"]
[null,null,"TWLアプリ"]
[]
[null,"SRL署名確認",null,"確認用SRL","結果","確認"]
[null,null,"ユーザーアプリ　正常","user.srl","○","○"]
[null,null,"ユーザーアプリ　ヘッダ異常","user_headerbreak.srl","×","○"]
[null,null,"ユーザーアプリ　ARM9 static異常","user_arm9flxbreak.srl","×","○"]
[null,null,"ユーザーアプリ　ARM9 static.LTD異常","user_arm9ltdbreak.srl","×","○"]
[null,null,"ユーザーアプリ　ARM7 static異常","user_arm7flxbreak.srl","×","○"]
[null,null,"ユーザーアプリ　ARM7 static.LTD異常","user_arm7ltdbreak.srl","×","○"]
[null,null,"システムアプリ　正常","system.srl","○","○"]
[null,null,"システムアプリ　ヘッダ異常","system_headerbreak.srl","×","○"]
[null,null,"システムアプリ　ARM9 static異常","system_arm9flxbreak.srl","×","○"]
[null,null,"システムアプリ　ARM9 static.LTD異常","system_arm9ltdbreak.srl","×","○"]
[null,null,"システムアプリ　ARM7 static異常","system_arm7flxbreak.srl","×","○"]
[null,null,"システムアプリ　ARM7 static.LTD異常","system_arm7ltdbreak.srl","×","○"]
[null,null,"セキュアアプリ　正常","secure.srl","○","○"]
[null,null,"セキュアアプリ　ヘッダ異常","secure_headerbreak.srl","×","○"]
[null,null,"セキュアアプリ　ARM9 static異常","secure_arm9flxbreak.srl","×","○"]
[null,null,"セキュアアプリ　ARM9 static.LTD異常","secure_arm9ltdbreak.srl","×","○"]
[null,null,"セキュアアプリ　ARM7 static異常","secure_arm7flxbreak.srl","×","○"]
[null,null,"セキュアアプリ　ARM7 static.LTD異常","secure_arm7ltdbreak.srl","×","○"]
[]
[null,"SRL-AES確認",null,"確認用SRL","SRL","TLF"]
[null,null,"NANDファーム",null,"○"]
[null,null,"ランチャー"]
[]
[null,"SCFGレジスタ値"]
[null,"WRAM設定"]
[]
[{"$nulls":6},"FS","FS","FS","LCFG","FS","FS","FS","FS","FS","FS","FS","FS","FS","SDK-API","FS"]
[null,"マウント情報",null,"確認用SRL","マウント情報","パーミッション","nand:/","nand2:/","content:/","shared1:/","shared2:/","photo:/","dataPub:/","dataPrv:/","sdmc:/","nand:/\nsys","nand:/\nimport","nand:/\ntmp","<srl>","<banner>","<tmpjump>"]
[null,"パーミッション","カード　ユーザーアプリ　SDなし　NANDなし","RomTypeTest0.srl",null,"○","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,"カード　ユーザーアプリ　SDなし　NANDあり","RomTypeTest1.srl",null,"△","NA","NA","-","RO","RW","RW","-","-","-","-","-","-","-","-","RW","ランチャーのバグ。カードブートの時、shared1をマウントしないので、shared1にアクセスできない。\nカードブートの時にTMPJUMPにアクセスできないのは、仕様変更の必要あり。"]
[null,null,"カード　ユーザーアプリ　SDあり　NANDあり","RomTypeTest2.srl",null,"△","NA","NA","-","RO","RW","RW","-","-","RW","-","-","-","-","-","RW","同上"]
[null,null,"カード　システムセキュアアプリ　SDなし　NANDあり","RomTypeTest3.srl",null,"○","RW","RW","-","RO","RW","RW","-","-","-","RW","RW","RW","-","-","RW"]
[null,null,"カード　システムセキュアアプリ　SDあり　NANDあり","RomTypeTest4.srl",null,"○","RW","RW","-","RO","RW","RW","-","-","RW","RW","RW","RW","-","-","RW"]
[null,null,"NAND　ユーザーアプリ　SDなし　PUBなし　PRVなし","RT5A.Release.tad",null,"△","NA","NA","RO","RO","RW","RW","-","-","-","-","-","-","RO","RW","RW","<srl>をWriteModeでオープンできてしまう。"]
[null,null,"NAND　ユーザーアプリ　SDなし　PUBなし　PRVあり","RT6A.Release.tad",null,"△","NA","NA","RO","RO","RW","RW","-","RW","-","-","-","-","RO","RW","RW","同上"]
[null,null,"NAND　ユーザーアプリ　SDなし　PUBあり　PRVなし","RT7A.Release.tad",null,"△","NA","NA","RO","RO","RW","RW","RW","-","-","-","-","-","RO","RW","RW","同上"]
[null,null,"NAND　ユーザーアプリ　SDなし　PUBあり　PRVあり","RT8A.Release.tad",null,"△","NA","NA","RO","RO","RW","RW","RW","RW","-","-","-","-","RO","RW","RW","同上"]
[null,null,"NAND　ユーザーアプリ　SDあり　PUBなし　PRVなし","RT9A.Release.tad",null,"△","NA","NA","RO","RO","RW","RW","-","-","RW","-","-","-","RO","RW","RW","同上"]
[null,null,"NAND　ユーザーアプリ　SDあり　PUBなし　PRVあり","RTaA.Release.tad",null,"△","NA","NA","RO","RO","RW","RW","-","RW","RW","-","-","-","RO","RW","RW","同上"]
[null,null,"NAND　ユーザーアプリ　SDあり　PUBあり　PRVなし","RTbA.Release.tad",null,"△","NA","NA","RO","RO","RW","RW","RW","-","RW","-","-","-","RO","RW","RW","同上"]
[null,null,"NAND　ユーザーアプリ　SDあり　PUBあり　PRVあり","RTcA.Release.tad",null,"△","NA","NA","RO","RO","RW","RW","RW","RW","RW","-","-","-","RO","RW","RW","同上"]
[null,null,"NAND　システムアプリ　SDなし　PRVなし","RTdA.Release.tad",null,"△","NA","NA","RO","RO","RW","RW","-","-","-","-","-","-","RO","RW","RW","同上"]
[null,null,"NAND　システムアプリ　SDなし　PRVあり","RTeA.Release.tad",null,"△","NA","NA","RO","RO","RW","RW","-","RW","-","-","-","-","RO","RW","RW","同上"]
[null,null,"NAND　システムアプリ　SDあり　PRVなし","RTfA.Release.tad",null,"△","NA","NA","RO","RO","RW","RW","-","-","RW","-","-","-","RO","RW","RW","同上"]
[null,null,"NAND　システムアプリ　SDあり　PRVあり","RTgA.Release.tad",null,"△","NA","NA","RO","RO","RW","RW","-","RW","RW","-","-","-","RO","RW","RW","同上"]
[null,null,"NAND　システムセキュアアプリ　SDなし　PRVなし","RThA.Release.tad",null,"△","RW","RW","RO","RO","RW","RW","-","-","-","RW","RW","RW","RO","RW","RW","同上"]
[null,null,"NAND　システムセキュアアプリ　SDなし　PRVあり","RTiA.Release.tad",null,"△","RW","RW","RO","RO","RW","RW","-","RW","-","RW","RW","RW","RO","RW","RW","同上"]
[null,null,"NAND　システムセキュアアプリ　SDあり　PRVなし","RTjA.Release.tad",null,"△","RW","RW","RO","RO","RW","RW","-","-","RW","RW","RW","RW","RO","RW","RW","同上"]
[null,null,"NAND　システムセキュアアプリ　SDあり　PRVあり","RTkA.Release.tad",null,"△","RW","RW","RO","RO","RW","RW","-","RW","RW","RW","RW","RW","RO","RW","RW","同上"]
[]
[null,"アプリジャンプ",null,null,"動作"]
[null,null,"ノーマルジャンプ","TwlSDK/build/demos.TWL/nandApp/launcher_param/AppliCooperation","○"]
[null,null,"TMPジャンプ","TwlSDK/build/demos.TWL/nandApp/launcher_param/ExecTmpApp","○"]
[]
[null,"TitleIDリスト",null,"確認用SRL","確認"]
[null,null,"アプリジャンプ"]
[null,null,"PrvDataマウント"]
[null,null,"PubDataマウント"]
[]
[null,"鍵引渡し",null,"確認用SRL","開発用鍵","製品用鍵"]
[null,null,"commonKey",null,"○"]
[null,null,"デバッガランチャー用commonKey",null,"○"]
[null,null,"AES SlotB ES用Seed",null,"○"]
[null,null,"AES SlotB NAM用Seed",null,"○"]
[null,null,"AES Slot B"]
[null,null,"AES Slot C"]
[]
[null,"バナー",null,"確認用SRL","確認"]
[null,null,"TWLバナー（アニメ）","TwlIPL/build/systemMenu_RED/PictoChat","○"]
[null,null,"サブバナー","TwlSDK/build/demos.TWL/nandApp/SubBanner","○"]
[]
[null,"固定情報ロード",null,"確認用SRL","確認"]
[null,null,"HWセキュア情報","TwlIPL/build/tests/CheckPreloadParamters","○"]
[null,null,"HWノーマル情報","TwlIPL/build/tests/CheckPreloadParamters","○"]
[null,null,"TWL本体設定","TwlIPL/build/tests/CheckPreloadParamters","○"]
[]
[null,"本体設定",null,"確認用SRL","確認"]
[null,null,"各種設定","MachineSettings.srl","○"]
[]
[null,"NandInitializer",null,"確認用SRL","確認"]
[null,null,"NANDフォーマット",null,"○"]
[null,null,"リージョン変更",null,"○"]
[]
[null,"ランチャー書き込み",null,"確認用SRL","動作"]
[null,null,"sdmc-launcher + NandInitializerProduction"]

{"sheet":"実機","index":1,"n_rows":99,"n_cols":19,"rows_kept":99,"flags":["formulas_cached_only"]}
[]
[null,"実機確認"]
[]
[]
[null,"アプリブート確認",null,"確認用SRL","カード\nブート","NANDブート"]
[null,null,"NTRアプリ",null,"○"]
[null,null,"TWL-HYBアプリ",null,"○","○"]
[null,null,"TWL-LTDアプリ",null,"○","○"]
[]
[null,"アプリロード範囲確認",null,"確認用SRL","確認"]
[null,null,"NTRアプリ"]
[null,null,"TWLアプリ"]
[]
[null,"アプリ再配置確認",null,"確認用SRL","確認"]
[null,null,"NTRアプリ"]
[null,null,"TWLアプリ"]
[]
[null,"SRL署名確認",null,"確認用SRL","結果","確認"]
[null,null,"ユーザーアプリ　正常","user.srl","○","○"]
[null,null,"ユーザーアプリ　ヘッダ異常","user_headerbreak.srl","×","○"]
[null,null,"ユーザーアプリ　ARM9 static異常","user_arm9flxbreak.srl","×","○"]
[null,null,"ユーザーアプリ　ARM9 static.LTD異常","user_arm9ltdbreak.srl","×","○"]
[null,null,"ユーザーアプリ　ARM7 static異常","user_arm7flxbreak.srl","×","○"]
[null,null,"ユーザーアプリ　ARM7 static.LTD異常","user_arm7ltdbreak.srl","×","○"]
[null,null,"システムアプリ　正常","system.srl","○","○"]
[null,null,"システムアプリ　ヘッダ異常","system_headerbreak.srl","×","○"]
[null,null,"システムアプリ　ARM9 static異常","system_arm9flxbreak.srl","×","○"]
[null,null,"システムアプリ　ARM9 static.LTD異常","system_arm9ltdbreak.srl","×","○"]
[null,null,"システムアプリ　ARM7 static異常","system_arm7flxbreak.srl","×","○"]
[null,null,"システムアプリ　ARM7 static.LTD異常","system_arm7ltdbreak.srl","×","○"]
[null,null,"セキュアアプリ　正常","secure.srl","○","○"]
[null,null,"セキュアアプリ　ヘッダ異常","secure_headerbreak.srl","×","○"]
[null,null,"セキュアアプリ　ARM9 static異常","secure_arm9flxbreak.srl","×","○"]
[null,null,"セキュアアプリ　ARM9 static.LTD異常","secure_arm9ltdbreak.srl","×","○"]
[null,null,"セキュアアプリ　ARM7 static異常","secure_arm7flxbreak.srl","×","○"]
[null,null,"セキュアアプリ　ARM7 static.LTD異常","secure_arm7ltdbreak.srl","×","○"]
[]
[null,"SRL-AES確認",null,"確認用SRL","SRL","TLF"]
[null,null,"NANDファーム",null,"○"]
[null,null,"ランチャー"]
[]
[null,"SCFGレジスタ値"]
[null,"WRAM設定"]
[]
[]
[null,"マウント情報",null,"確認用SRL","マウント情報","パーミッション","nand:/","nand2:/","content:/","shared1:/","shared2:/","photo:/","dataPub:/","dataPrv:/","sdmc:/","nand:/\nsys","nand:/\nimport","nand:/\ntmp"]
[null,"パーミッション","カード　ユーザーアプリ　SDなし　NANDなし",{"$nulls":3},"-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,"カード　ユーザーアプリ　SDなし　NANDあり",{"$nulls":3},"NA","NA","-","RO","RW","RW","-","-","-","-","-","-"]
[null,null,"カード　ユーザーアプリ　SDあり　NANDあり",{"$nulls":3},"NA","NA","-","RO","RW","RW","-","-","RW","-","-","-","※今のコードでは、SDMCを有効にしたら、カードアクセスも有効になるので、\"SDあり、NANDなし”の組み合わせはない。"]
[null,null,"カード　システムセキュアアプリ　SDなし　NANDあり",{"$nulls":3},"RW","RW","-","RO","RW","RW","-","-","-","RW","RW","RW"]
[null,null,"カード　システムセキュアアプリ　SDあり　NANDあり",{"$nulls":3},"RW","RW","-","RO","RW","RW","-","-","RW","RW","RW","RW"]
[null,null,"NAND　ユーザーアプリ　SDなし　PUBなし　PRVなし",{"$nulls":3},"NA","NA","RO","RO","RW","RW","-","-","-","-","-","-"]
[null,null,"NAND　ユーザーアプリ　SDなし　PUBなし　PRVあり",{"$nulls":3},"NA","NA","RO","RO","RW","RW","-","RW","-","-","-","-"]
[null,null,"NAND　ユーザーアプリ　SDなし　PUBあり　PRVなし",{"$nulls":3},"NA","NA","RO","RO","RW","RW","RW","-","-","-","-","-"]
[null,null,"NAND　ユーザーアプリ　SDなし　PUBあり　PRVあり",{"$nulls":3},"NA","NA","RO","RO","RW","RW","RW","RW","-","-","-","-"]
[null,null,"NAND　ユーザーアプリ　SDあり　PUBなし　PRVなし",{"$nulls":3},"NA","NA","RO","RO","RW","RW","-","-","RW","-","-","-"]
[null,null,"NAND　ユーザーアプリ　SDあり　PUBなし　PRVあり",{"$nulls":3},"NA","NA","RO","RO","RW","RW","-","RW","RW","-","-","-"]
[null,null,"NAND　ユーザーアプリ　SDあり　PUBあり　PRVなし",{"$nulls":3},"NA","NA","RO","RO","RW","RW","RW","-","RW","-","-","-"]
[null,null,"NAND　ユーザーアプリ　SDあり　PUBあり　PRVあり",{"$nulls":3},"NA","NA","RO","RO","RW","RW","RW","RW","RW","-","-","-"]
[null,null,"NAND　システムアプリ　SDなし　PRVなし",{"$nulls":3},"NA","NA","RO","RO","RW","RW","-","-","-","-","-","-"]
[null,null,"NAND　システムアプリ　SDなし　PRVあり",{"$nulls":3},"NA","NA","RO","RO","RW","RW","-","RW","-","-","-","-"]
[null,null,"NAND　システムアプリ　SDあり　PRVなし",{"$nulls":3},"NA","NA","RO","RO","RW","RW","-","-","RW","-","-","-"]
[null,null,"NAND　システムアプリ　SDあり　PRVあり",{"$nulls":3},"NA","NA","RO","RO","RW","RW","-","RW","RW","-","-","-"]
[null,null,"NAND　システムセキュアアプリ　SDなし　PRVなし",{"$nulls":3},"RW","RW","RO","RO","RW","RW","-","-","-","RW","RW","RW"]
[null,null,"NAND　システムセキュアアプリ　SDなし　PRVあり",{"$nulls":3},"RW","RW","RO","RO","RW","RW","-","RW","-","RW","RW","RW"]
[null,null,"NAND　システムセキュアアプリ　SDあり　PRVなし",{"$nulls":3},"RW","RW","RO","RO","RW","RW","-","-","RW","RW","RW","RW"]
[null,null,"NAND　システムセキュアアプリ　SDあり　PRVあり",{"$nulls":3},"RW","RW","RO","RO","RW","RW","-","RW","RW","RW","RW","RW"]
[]
[null,"アプリジャンプ",null,"確認用SRL","動作"]
[null,null,"ノーマルジャンプ",null,"○"]
[null,null,"TMPジャンプ",null,"○"]
[]
[null,"TitleIDリスト",null,"確認用SRL","確認"]
[null,null,"アプリジャンプ"]
[null,null,"PrvDataマウント"]
[null,null,"PubDataマウント"]
[]
[null,"鍵引渡し",null,"確認用SRL","開発用鍵","製品用鍵"]
[null,null,"commonKey"]
[null,null,"デバッガランチャー用commonKey"]
[null,null,"AES SlotB ES用Seed"]
[null,null,"AES SlotB NAM用Seed"]
[null,null,"AES Slot B"]
[null,null,"AES Slot C"]
[]
[null,"固定情報ロード",null,"確認用SRL","確認"]
[null,null,"HWセキュア情報"]
[null,null,"HWノーマル情報"]
[null,null,"TWL本体設定"]
[]
[null,"本体設定",null,"確認用SRL","確認"]
[null,null,"各種設定",null,"○"]
[]
[null,"NandInitializer",null,"確認用SRL","確認"]
[null,null,"NANDフォーマット",null,"○"]
[null,null,"リージョン変更",null,"○"]
[]
[null,"ランチャー書き込み",null,"確認用SRL","動作"]
[null,null,"sdmc-launcher + NandInitializerProduction",null,"○"]