{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["値の書き換え","基本操作","MRC機能"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"値の書き換え","index":0,"n_rows":34,"n_cols":17,"rows_kept":34,"merged":[[7,1,7,10],[19,1,19,16],[30,0,30,1],[30,2,30,3],[31,0,31,1],[32,0,32,1],[33,0,33,1]],"flags":["formulas_cached_only"]}
["マスタエディタ デバッグ項目 (書き換えチェック編)"]
[]
["○リージョンが選択されるか"]
["リージョン","日本","米国","欧州","豪州","欧+豪","オール"]
["バイナリ","00000001","00000002","00000004","00000008","0000000C","FFFFFFFF"]
[]
["○ペアレンタルコントロールの値がセットできるか"]
["団体","バイナリチェック"]
["CERO","全年齢(80h)","12(8Ch)","15(8Fh)","17(91h)","18(92h)",null,"審査中(C0h)"]
["ESRB","制限なし(80h)","3(83h)","6(86h)","10(8Ah)","13(8Dh)","17(91h)","審査中(C0h)"]
["USK","全年齢(80h)","7(86h)","12(8Ch)","16(90h)","18(92h)",null,"審査中(C0h)"]
["PEGI","制限なし(80h)","3(83h)","7(87h)","12(8Ch)","16(90h)","18(92h)","審査中(C0h)"]
["PEGI_PRT","制限なし(80h)","4(84h)","6(86h)","12(8Ch)","16(90h)","18(92h)","審査中(C0h)"]
["PEGI_BBFC","制限なし(80h)","3(83h)","4(84h)","7(87h)","8(88h)","12(8Ch)","15(8Fh)","16(90h)","18(92h)","審査中(C0h)"]
["OFLC","G(80h)","PG(87h)","M(8Eh)","MA(8Fh)",null,null,"審査中(C0h)"]
[]
[{"$nulls":4},"各リージョンのランチャー上で動作確認もする"]
[]
["○リージョンに含まれる団体は値がセットされて、含まれない団体は00hにクリアされるか"]
["リージョン","バイナリチェック"]
["日本","CERO","ESRB","予約","USK","PEGI","予約","PEGI_PRT","PEGI_BBFC","OFLC","予約(GRB)","予約","予約","予約","予約","予約","予約"]
["米国","CERO","ESRB","予約","USK","PEGI","予約","PEGI_PRT","PEGI_BBFC","OFLC","予約(GRB)","予約","予約","予約","予約","予約","予約"]
["欧州","CERO","ESRB","予約","USK","PEGI","予約","PEGI_PRT","PEGI_BBFC","OFLC","予約(GRB)","予約","予約","予約","予約","予約","予約"]
["豪州","CERO","ESRB","予約","USK","PEGI","予約","PEGI_PRT","PEGI_BBFC","OFLC","予約(GRB)","予約","予約","予約","予約","予約","予約"]
["欧州+豪州","CERO","ESRB","予約","USK","PEGI","予約","PEGI_PRT","PEGI_BBFC","OFLC","予約(GRB)","予約","予約","予約","予約","予約","予約"]
["オール","CERO","ESRB","予約","USK","PEGI","予約","PEGI_PRT","PEGI_BBFC","OFLC","予約(GRB)","予約","予約","予約","予約","予約","予約"]
[]
[{"$nulls":4},"値がセットされる団体"]
[]
["○フラグ"]
["フラグ名",null,"バイナリチェック",null,"動作確認"]
["EULAフラグ",null,"立つ","下りる"]
["ワイヤレスアイコン",null,"立つ","下りる"]
["Wi-Fiアイコン",null,"立つ","下りる"]

{"sheet":"基本操作","index":1,"n_rows":28,"n_cols":5,"rows_kept":28,"merged":[[19,1,19,4],[20,1,20,4],[21,1,21,4],[22,1,22,4],[23,1,23,4],[25,1,25,4],[26,1,26,4],[27,1,27,4]],"flags":["formulas_cached_only"]}
["マスタエディタ デバッグ項目 (基本操作編)"]
[]
["[正常系]"]
[]
["○出力ファイルの保存/読み込みができるかテスト"]
[null,"デスクトップ","マイドキュメント","C:\\","C:\\保存先"]
["SRL保存のみ"]
["提出書保存のみ"]
["両方の保存"]
["SRLの読み込み(メニュー)"]
["SRLの読み込み(ドラッグ)"]
[]
["○一時ファイルの保存/読み込みができるかテスト"]
[null,"デスクトップ","マイドキュメント","C:\\","C:\\保存先"]
["保存"]
["読み込み"]
[]
[]
["[異常系]"]
["操作","チェック項目"]
["SRLの保存のみ","読み込んだSRLがなくなったときSRLの書き込み失敗ダイアログが出るか"]
["両方の保存","上と同じ"]
["提出書保存のみ","読み込んだSRLがなくなったとき提出書の書き込み失敗ダイアログが出るか"]
["提出書保存のみ","提出書を開いている最中に上書きしたとき書き込み失敗ダイアログが出るか"]
["両方の保存","上と同じ"]
["一時ファイルの読み込み","一時ファイルに記載したSRLがなくなったときに警告ダイアログが出るか"]
["一時ファイルの保存","SRLを読み込んでいないときに一時ファイルの保存ができるか"]
["一時ファイルの読み込み","上記の一時ファイルを読み込むことができるか"]

{"sheet":"MRC機能","index":2,"n_rows":64,"n_cols":5,"rows_kept":64,"merged":[[2,0,3,0],[2,4,3,4],[4,0,6,0],[4,4,11,4],[7,0,8,0],[11,0,12,0],[13,4,18,4],[19,0,23,0],[20,4,40,4],[25,0,27,0],[29,0,34,0],[39,0,41,0],[42,0,47,0],[42,4,49,4],[50,0,51,0],[51,4,63,4],[52,0,53,0],[54,0,55,0],[56,0,57,0],[58,0,59,0],[60,0,61,0],[62,0,63,0]],"flags":["formulas_cached_only"]}
["○マスタエディタ デバッグ項目 (MRC機能編)"]
["チェック項目","対象srlメディア","デバッグ用不正ソフトのつくりかた","デバッグ用不正ソフト名","どうなったらいいのか"]
["エラーがでないこと","Card","何もしない","regular_card1.srl","エラーが何も表示されない"]
[null,"NAND","何もしない","regular_nand1.srl"]
["ソフトタイトル","Card","小文字が含まれている","title_name_card1.srl","エラー表示"]
[null,"Card","スペースが00hになっている","title_name_card2.srl"]
[null,"Card","末尾がスペースで埋められている","title_name_card3.srl"]
["イニシャルコード","Card","小文字が含まれている","game_code_card1.srl"]
[null,"Card","SDKのデモ(NTRJ)を使用する","game_code_card2.srl"]
["メーカーコード","Card","小文字が含まれている","maker_code_card1.srl"]
["デバイスタイプ","Card/NAND","01hとなっている","device_type_card1.srl"]
["リマスターバージョン","Card/NAND","0Ahとなっている","rom_version_card1.srl"]
[null,"Card/NAND","E0hとなっている","rom_version_card2.srl","エラーは表示されず、\nバージョンが\"E\"となる。"]
["バナーオフセット","Card/NAND","00000000hとなっている","banner_offset_card1.srl","エラー表示"]
["キャラクターデータCRC","Card/NAND","0000hとなっている","logo_crc_card1.srl"]
["ROMヘッダCRC","Card/NAND","0000hとなっている","header_crc_card1.srl"]
["ROM実行サイズ","Card/NAND","0000hとなっている","valid_size_card1.srl"]
["システムコールライブラリ","Card/NAND","SDKのデモを使用する","syscall_card1.srl"]
["プラットフォーム","Card/NAND","NTR専用ソフトに署名をつける","platform_card1.srl"]
["デバイス容量","Card","256MbitのファイルのROMサイズに512Mbitを指定する","rom_size_card1.srl","警告"]
[null,"Card","512MbitのファイルのROMサイズに256Mbitを指定する","rom_size_card2.srl","エラー表示"]
[null,"Card","128Mbitを指定する","rom_size_card3.srl"]
[null,"Card","8Gbitを指定する","rom_size_card4.srl"]
[null,"NAND","512MBitを指定する","rom_size_nand1.srl"]
["ROMコントロール情報","Card/NAND","MROM設定にする","mrom_card1.srl"]
["TWL ROMオフセット","Card","ノーマル領域ROMオフセット(NA)を0","rom_offset_card1.srl"]
[null,"Card","セキュア領域ROMオフセット(KA)を0","rom_offset_card2.srl"]
[null,"Card","NA = 2h と KA = 1h","rom_offset_card3.srl"]
["リージョン","Card/NAND","日米両方を立てる","region_card1.srl"]
["アクセスコントロール情報","NAND","第5bitと第8bitを同時に立てる","access_control_nand1.srl"]
[null,"Card","第5bitを立てる","access_control_card1.srl"]
[null,"Card","第8bitを立てる","access_control_card2.srl"]
[null,"Card","第3bitを立てる","access_control_card3.srl"]
[null,"Card","第4bitを立てる","access_control_card4.srl"]
[null,"NAND","DSサウンドの第6bitを下げる","access_control_nand2.srl"]
["SCFG設定","Card/NAND","第31bitを立てる","scfg_card1.srl"]
["アイコン表示フラグ","Card","第3bitと第4bitを同時に立てる","icon_flag_card1.srl"]
["TitleID Lo","Card/NAND","20080911版のPictoChatを使用する","titleid_lo_nand1.srl"]
["アプリ種別","Card/NAND","UIGランチャーの署名をユーザにする","apptype_nand1.srl"]
["実ファイルサイズ","Card","1バイト削る","file_size_card1.srl"]
[null,"NAND","DSサウンドのPublicセーブデータと\nPrivateセーブデータをともに1000000(16MB)にする","file_size_nand1.srl"]
[null,"NAND","DSサウンドのPublicセーブデータと\nPrivateセーブデータをともに0800000(8MB)にする","file_size_nand2.srl","エラーなし"]
["SI-Frash対応","Card","1Gbitの最終20Mbitの先頭をFEhにする","padding_card1.srl","エラー表示"]
[null,"Card","1Gbitの最終20Mbitの終端をFEhにする","padding_card2.srl"]
[null,"Card","2Gbitの最終40Mbitの先頭をFEhにする","padding_card3.srl"]
[null,"Card","2Gbitの最終40Mbitの終端をFEhにする","padding_card4.srl"]
[null,"Card","4Gbitの最終83Mbitの先頭をFEhにする","padding_card5.srl"]
[null,"Card","4Gbitの最終83Mbitの終端をFEhにする","padding_card6.srl"]
["セグメント3CRC","Card","3FFFhを変更する","seg3crc_card1.srl"]
["バナー","Card/NAND","漢字を埋め込む","banner_card1.srl"]
["クローンブート署名","Card/NAND","署名を埋め込んだsrlを使用する","clone_boot_card1.srl","エラーなし\n特記事項に表示"]
[null,"Card/NAND","RC2よりも前でビルドしたsrlに署名を埋め込む","clone_boot_card2.srl","エラー表示"]
["予約領域[78h-7Fh]","Card/NAND","78hが01h","reserved_card01.srl"]
[null,"Card/NAND","7Ｆhが01h","reserved_card02.srl"]
["予約領域[160h-17Fh]","Card/NAND","160hが01h","reserved_card03.srl"]
[null,"Card/NAND","17Fhが01h","reserved_card04.srl"]
["予約領域[15h, 1Bh]","Card/NAND","15hが01h","reserved_card05.srl"]
[null,"Card/NAND","1Bhが01h","reserved_card06.srl"]
["予約領域[99h,BFh]","Card/NAND","99hが01h","reserved_card07.srl"]
[null,"Card/NAND","BFhが01h","reserved_card08.srl"]
["予約領域[240h,2EFh]","Card/NAND","240hが01h","reserved_card09.srl"]
[null,"Card/NAND","2EFhが01h","reserved_card10.srl"]
["予約領域[378h,F7Fh]","Card/NAND","378hが01h","reserved_card11.srl"]
[null,"Card/NAND","F7Fhが01h","reserved_card12.srl"]