{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["MRC機能"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"MRC機能","index":0,"n_rows":103,"n_cols":6,"rows_kept":103,"merged":[[4,0,5,0],[4,4,5,4],[6,0,8,0],[6,4,13,4],[9,0,10,0],[13,0,14,0],[15,0,16,0],[17,4,22,4],[23,0,27,0],[23,5,26,5],[24,4,29,4],[29,0,30,0],[29,1,30,1],[31,0,32,0],[33,0,35,0],[33,4,44,4],[36,0,37,0],[38,0,47,0],[46,4,49,4],[48,0,50,0],[48,1,50,1],[52,4,53,4],[56,0,59,0],[59,4,67,4],[60,0,65,0],[60,5,65,5],[68,0,69,0],[69,4,70,4],[70,0,71,0],[72,4,82,4],[73,0,77,0],[80,0,81,0],[80,1,81,1],[82,0,86,0],[82,1,86,1],[84,4,85,4],[87,0,88,0],[87,4,102,4],[89,0,90,0],[91,0,92,0],[93,0,94,0],[95,0,96,0],[97,0,98,0],[99,0,100,0],[101,0,102,0]],"flags":["formulas_cached_only"]}
["○マスタエディタ デバッグ項目 (MRC機能編)"]
["カードアプリとNANDアプリ共通のチェック項目はカードアプリのみでチェック(両方作成するのがしんどいので)",{"$nulls":3},"新規追加"]
[]
["チェック項目","対象srlメディア","デバッグ用不正ソフトのつくりかた","デバッグ用不正ソフト名","どうなったらいいのか","備考"]
["エラーがでないこと","Card","何もしない(正常)","regular_card1.srl","エラー表示なし"]
[null,"NAND","何もしない(正常)","regular_nand1.srl/.tad"]
["ソフトタイトル","Card","小文字が含まれている","title_name_card1.srl","エラー表示"]
[null,"Card","スペースが00hになっている","title_name_card2.srl"]
[null,"Card","末尾がスペースで埋められている","title_name_card3.srl"]
["イニシャルコード","Card","小文字が含まれている","game_code_card1.srl"]
[null,"Card","SDKのデモ(NTRJ)を使用する","game_code_card2.srl"]
["メーカーコード","Card","小文字が含まれている","maker_code_card1.srl"]
["デバイスタイプ","Card/NAND","01hとなっている","device_type_card1.srl"]
["リマスターバージョン","Card/NAND","10hとなっている","rom_version_card1.srl"]
[null,"Card/NAND","E0hとなっている","rom_version_card2.srl","エラーは表示されず、\nバージョンが\"E\"となる。"]
["RomSpeedType","Card","カードアプリなのにRomSpeedTypeが設定されていない","rom_speed_type_card1.srl","エラー表示"]
[null,"NAND","NANDアプリでRomSpeedTypeが設定されていない","rom_speed_type_nand1.srl","エラーなし"]
["バナーオフセット","Card/NAND","00000000hとなっている","banner_offset_card1.srl","エラー表示"]
["キャラクターデータCRC","Card/NAND","0000hとなっている","logo_crc_card1.srl"]
["ROMヘッダCRC","Card/NAND","0000hとなっている","header_crc_card1.srl"]
["ROM実効サイズ","Card/NAND","0000hとなっている","valid_size_card1.srl"]
["システムコールライブラリ","Card/NAND","SDKのデモを使用する","syscall_card1.srl"]
["プラットフォーム","Card/NAND","NTR専用ソフトに署名をつける","platform_card1.srl"]
["デバイス容量","Card","256MbitのファイルのROMサイズに512Mbitを指定する","rom_size_card1.srl","警告","サイズが大きいので\n西川がローカルで所有"]
[null,"Card","512MbitのファイルのROMサイズに256Mbitを指定する","rom_size_card2.srl","エラー表示"]
[null,"Card","128Mbitを指定する","rom_size_card3.srl"]
[null,"Card","8Gbitを指定する","rom_size_card4.srl"]
[null,"NAND","512MBitを指定する","rom_size_nand1.srl"]
["ROMコントロール情報","Card/NAND","MROM設定にする","mrom_card1.srl"]
["デバッガ動作禁止フラグ","Card/NAND","ユーザアプリの第3bitを立てる","disable_debug_card_usr1.srl"]
[null,null,"システムアプリの第3bitを下ろす","disable_debug_nand_sys1.srl","警告"]
["ノーマルジャンプ許可","Card/NAND","ユーザアプリの第0bitを立てる","normal_jump_card_usr1.srl","エラー表示"]
[null,"NAND","システムアプリの第0bitを立てる","normal_jump_nand_sys1.srl","エラーは表示されず、\nノーマルジャンプ許可に\nチェックが入る"]
["TWL ROMオフセット","Card","ノーマル領域ROMオフセット(NA)を0","rom_offset_card1.srl","エラー表示"]
[null,"Card","セキュア領域ROMオフセット(KA)を0","rom_offset_card2.srl"]
[null,"Card","NA = 2h と KA = 1h","rom_offset_card3.srl"]
["リージョン","Card/NAND","日米両方を立てる","region_card1.srl"]
[null,"Card/NAND","ユーザアプリなのにオールリージョン","region_card2.srl"]
["アクセスコントロール情報","Card/NAND","ユーザカードアプリの第3bitを立てる","access_card_usr1.srl"]
[null,"Card","ユーザカードアプリの第4bitを立てる","access_card_usr2.srl"]
[null,"Card/NAND","ユーザカードアプリの第6bitを立てる","access_card_usr3.srl"]
[null,"Card/NAND","ユーザカードアプリの第5bitを立てる","access_card_usr4.srl"]
[null,"Card/NAND","ユーザカードアプリの第2bitを立てる","access_card_usr5.srl"]
[null,"Card","ユーザカードアプリの第10bitを立てる","access_card_usr6.srl"]
[null,"NAND","ユーザNANDアプリの第3bitを立てる","access_nand_usr1.srl"]
[null,"NAND","ユーザNANDアプリの第10bitを立てる","access_nand_usr2.srl","エラーが表示されない"]
[null,"NAND","DSサウンドの第5bitと第8bitを同時に立てる","access_nand_sys1.srl","エラー表示"]
[null,"NAND","DSサウンドの第6bitを下げる","access_nand_sys2.srl"]
["Shared2ファイルサイズ","Card/NAND","アクセスコントロール情報の第6bitを立てずに\nShared2ファイル5のサイズを2MBに設定する","shared2_card1.srl"]
[null,null,"アクセスコントロール情報の第6bitを立てて\nShared2ファイル0～5のサイズを0に設定する","shared2_card2.srl"]
[null,null,"アクセスコントロール情報の第6bitを立てて\n各Shared2ファイルのサイズを2MBに設定する","shared2_file*_card1.srl","設定ファイルの指定によっては\nエラーが表示される"]
["SCFG設定","Card/NAND","第31bitを立てる","scfg_card1.srl","警告"]
["NTRホワイトリストフラグ","Card/NAND","第6bitを立てる","whitelist.srl","エラー表示"]
["アイコン表示フラグ","Card","第3bitと第4bitを同時に立てる","icon_flag_card1.srl"]
["TitleID Lo","Card/NAND","20080911版のPictoChatを使用する","titleid_lo_nand1.srl","警告"]
["アプリ種別","Card/NAND","UIGランチャーの署名をユーザにする","apptype_nand1.srl","エラー表示"]
["実ファイルサイズ","Card","1バイト削る","file_size_card1.srl","警告"]
[null,"NAND","DSサウンドのPublicセーブデータと\nPrivateセーブデータをともに1000000(16MB)にする","file_size_nand1.srl","エラー表示"]
[null,"NAND","DSサウンドのPublicセーブデータと\nPrivateセーブデータをともに0800000(8MB)にする","file_size_nand2.srl","エラーなし"]
[null,"NAND","ユーザアプリのPubilcセーブデータと\nPrivateセーブデータとともに0800000(8MB)にする","file_size_nand3.srl","エラー表示"]
["SI-Frash対応","Card","1Gbitの最終20Mbitの先頭をFEhにする","padding_card1.srl",null,"サイズが大きいので\n西川がローカルで所有"]
[null,"Card","1Gbitの最終20Mbitの終端をFEhにする","padding_card2.srl"]
[null,"Card","2Gbitの最終40Mbitの先頭をFEhにする","padding_card3.srl"]
[null,"Card","2Gbitの最終40Mbitの終端をFEhにする","padding_card4.srl"]
[null,"Card","4Gbitの最終83Mbitの先頭をFEhにする","padding_card5.srl"]
[null,"Card","4Gbitの最終83Mbitの終端をFEhにする","padding_card6.srl"]
["セグメント3CRC","Card","3FFFhを変更する","seg3crc_card1.srl"]
["バナー","Card/NAND","漢字を埋め込む","banner_card1.srl"]
["クローンブート署名","Card/NAND","署名を埋め込んだsrlを使用する","clone_boot_card1.srl","エラーが表示されない\n特記事項に表示"]
[null,"Card/NAND","RC2よりも前でビルドしたsrlに署名を埋め込む","clone_boot_card2.srl","エラー表示"]
["NANDアプリのHYBRID条件","NAND","ただのHYBRIDアプリ","hybrid_nand1.srl"]
[null,"NAND","HYBRIDアプリにクローンブート署名をつける","hybrid_cloneboot_nand1.srl","エラーが表示されない\n特記事項に表示"]
["NANDアプリのLIMITED条件","NAND","LIMITEDアプリにクローンブート署名をつける","limited_cloneboot_nand1.srl","エラー表示"]
["AES暗号","Card","AES暗号フラグが立っていない","aes_card1.srl"]
[null,"Card","AES領域のサイズが0","aes_card2.srl"]
[null,"NAND","AES暗号フラグが立っていない","aes_nand1.srl"]
[null,"NAND","AES領域のサイズが0","aes_nand2.srl"]
[null,"NAND","AES領域2のサイズが0","aes_nand3.srl"]
["拡張常駐モジュール","Card","TWL専用領域ROMオフセットを大きくする(01h⇒02h)","main_ltd_rom_offset_card1_f.srl"]
["Debug/Releaseビルド","Card/NAND","ReleaseビルドしたSRL","release_build.srl"]
["Public/Privateセーブデータ","Card","カードアプリにPublicセーブデータのサイズを指定する","public_save_data_card1.srl"]
[null,null,"カードアプリにPrivateセーブデータのサイズを指定する","private_save_data_card1.srl"]
["ペアレンタルコントロール","Card/NAND","日本リージョンなのに\nCEROのレーティングがない(すべての団体が00h)","pctl_card1.srl"]
[null,null,"日本リージョンなのに\nCEROとESRBのレーティング年齢が設定されている(80h)","pctl_card2.srl","エラーなし"]
[null,null,"CEROのレーティング年齢に14歳を指定(8Eh)","pctl_card3.srl","エラー表示"]
[null,null,"レーティング表示不要フラグが立っているのに\nCEROのレーティング年齢に12歳が指定されている(8Ch)","pctl_card4.srl"]
[null,null,"レーティング表示不要フラグが立っている\nCEROのレーティング値は80h","pctl_card5.srl","警告\n(「現在の入力を反映」を選択)"]
["予約領域[78h-7Fh]","Card/NAND","78hが01h","reserved_card01.srl","エラー表示"]
[null,"Card/NAND","7Ｆhが01h","reserved_card02.srl"]
["予約領域[160h-17Fh]","Card/NAND","160hが01h","reserved_card03.srl"]
[null,"Card/NAND","17Fhが01h","reserved_card04.srl"]
["予約領域[15h, 1Bh]","Card/NAND","15hが01h","reserved_card05.srl"]
[null,"Card/NAND","1Bhが01h","reserved_card06.srl"]
["予約領域[99h,BFh]","Card/NAND","99hが01h","reserved_card07.srl"]
[null,"Card/NAND","BFhが01h","reserved_card08.srl"]
["予約領域[240h,2EFh]","Card/NAND","240hが01h","reserved_card09.srl"]
[null,"Card/NAND","2EFhが01h","reserved_card10.srl"]
["予約領域[378h,39Fh]","Card/NAND","378hが01h","reserved_card11.srl"]
[null,"Card/NAND","39Fhが01h","reserved_card12.srl"]
["予約領域[3B4h,F7Fh]","Card/NAND","3B4hが01h","reserved_card13.srl"]
[null,"Card/NAND","F7Fhが01h","reserved_card14.srl"]
["予約領域[1BCh,1BEh]","Card/NAND","1BChが01h","reserved_card15.srl"]
[null,"Card/NAND","1BEhが01h","reserved_card16.srl"]