# Changes

## v0.9 - Initial Release (released 2018/04/26)

* Lists all disc images currently installed on the RVT-H system.
* Can find "deleted" images that aren't accessible on the RVT-H but are still
  present on the HDD, and has an option to undelete these images.
  * Can undelete any image deleted by rvtwriter, which only clears the
    bank table entry.
  * Can undelete Wii images that were "flushed" using the front-panel button.
    * GameCube images deleted this way cannot currently be undeleted.
* Extracts disc images from an RVT-H system or HDD image into a GCM file.
  * Supports optional recryption to convert a debug-encrypted image to retail
    encryption with fake-signed ticket and TMD.
* Signature verification for all Wii disc images. Indicates if the signature
  is valid, invalid, or fakesigned. (Game partition only at the moment.)
* Installation of GameCube and Wii disc images onto an RVT-H system. If
  importing a retail Wii disc image, it will automatically be re-signed and
  re-encrypted using the debug keys. (Update partitions will be removed, since
  retail updates won't work properly on RVT-H.)
  * Supported image formats: GCM, headered GCM, CISO, WBFS
  * Split WBFS is not currently supported. Combine the .wbfs and .wbfs1 files
    before processing.
* Standalone disc image re-signing to convert e.g. retail to debug, debug
  to retail, unencrypted to debug, etc. Conversion to retail will result
  in a fakesigned image.
* Querying all available RVT-H Reader devices to determine which device name
  is associated with which reader. (Linux with UDEV only at the moment.)

NOTE: Converting an unencrypted image to encrypted is not currently supported.
