{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["RSA鍵管理","AES使用方針"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"RSA鍵管理","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"flags":["formulas_cached_only"]}
[]
["TWL RSA鍵管理"]
[]
[]
[]
[null,"鍵No.","種別","格納場所","格納タイミング","用途","RAM上データ消去タイミング","ファイル名","ビット数"]
[null,0,"公開鍵","ARM9 内蔵ROM","チップ埋め込み","GCDファーム署名認証","GCDファームブート前(※1)","pubkey_gcd.sbin",1024]
[null,1,"公開鍵","ARM9 内蔵ROM","チップ埋め込み","NORファーム署名認証","NORファームブート前","pubkey_nor.sbin",1024]
[null,2,"公開鍵","ARM9 内蔵ROM","チップ埋め込み","NANDファーム署名認証","NANDファームブート前","pubkey_nand.sbin",1024]
[null,3,"公開鍵","ARM9 内蔵ROM","チップ埋め込み","ランチャー署名認証","ランチャーブート前","pubkey_9_0.der",1024]
[null,4,"公開鍵","ARM9 内蔵ROM","チップ埋め込み","製品アプリ署名認証","アプリブート前","pubkey_9_1.der",1024]
[null,5,"公開鍵","ARM9 内蔵ROM","チップ埋め込み",null,"ショップアプリ以外のアプリブート前","pubkey_9_2.der",1024]
[null,6,"公開鍵","ARM9 内蔵ROM","チップ埋め込み",null,"アプリブート前","pubkey_9_3.der",1024]
[null,7,"公開鍵","ARM9 内蔵ROM","チップ埋め込み",null,"アプリブート前","pubkey_9_4.der",1024]
[null,8,"公開鍵","ARM9 内蔵ROM","チップ埋め込み",null,"アプリブート前","pubkey_9_5.der",1024]
[null,9,"公開鍵","ARM9 内蔵ROM","チップ埋め込み",null,"アプリブート前","pubkey_9_6.der",1024]
[null,10,"公開鍵","ARM9 内蔵ROM","チップ埋め込み",null,"アプリブート前","pubkey_9_7.der",1024]
[null,11,"公開鍵","ARM7 内蔵ROM","チップ埋め込み",null,"アプリブート前","pubkey_7_0.der",1024]
[null,12,"公開鍵","ARM7 内蔵ROM","チップ埋め込み",null,"アプリブート前","pubkey_7_1.der",1024]
[null,13,"公開鍵","ARM7 内蔵ROM","チップ埋め込み",null,"アプリブート前","pubkey_7_2.der",1024]
[null,14,"公開鍵","ARM7 内蔵ROM","チップ埋め込み",null,"アプリブート前","pubkey_7_3.der",1024]
[null,null,"公開鍵","NANDファームSRL",null,"開発アプリ署名認証","ランチャーブート前",null,1024]
[null,15,"公開鍵","ショップアプリSRL\nNUP-SRL","生産工程","本体ID署名認証","ショップアプリ以外のアプリブート前",null,1024]
[null,16,"公開鍵","ランチャーSRL","生産工程","本体情報署名認証","アプリブート前",null,1024]
[]
[]
[null,null,"(※1)GCDファームブート時は、全ての鍵を消去している。"]
[]
[null,null,"BroadOnは4096bitくらいを考えている？"]
[null,null,"ルートCAキーはBroadOnの中で持つ。"]

{"sheet":"AES使用方針","index":1,"n_rows":13,"n_cols":17,"rows_kept":13,"merged":[[4,0,5,0],[4,1,5,1],[4,2,4,3],[4,4,4,6],[4,7,4,9],[4,10,4,12],[4,13,5,13],[4,14,5,14],[4,15,5,15],[4,16,5,16]],"flags":["formulas_cached_only"]}
[]
["TWL AES鍵管理"]
[]
[]
["鍵\nNo.","SDK KeyType","関連付け",null,"ID",null,null,"Seed",null,null,"RAW AES Key",null,null,"使用者","用途","使用者２","API公開"]
[null,null,"HWID","Game\nCode","アプリ\nセット可","セット値","セット者","アプリ\nセット可","セット値","セット者","アプリ\nセット可","セット値","セット者"]
[0,"AES_KEY_TYPE_APP","×","○","×","デフォルト値\n+GameCode","BootRom\n(GameCode部 4 or 8bytesのみランチャー)","　×","ROMヘッダ署名内のSeed","NANDファーム\nランチャー","×","ROMヘッダ署名内のSeed","ランチャー","NANDファーム\nランチャー","製品版SRL一部暗号\n開発版SRL一部暗号","アプリ管理画面","非公開"]
[1,"AES_KEY_TYPE_APP_HARD","○","○","×","デフォルト値\n+HWID\n+GameCode","BootRom\n(GameCode部 4 or 8 bytesのみランチャー)","×","???","AESライブラリ","×","-","-","AESライブラリ","AES_randで使う。","アプリ管理画面","非公開"]
[2,"AES_KEY_TYPE_RAW","×","×","×","デフォルト値","BootRom","×","-","-","○","任意の値","アプリ","アプリ",null,null,"公開"]
[3,"AES_KEY_TYPE_HARD","○","×","×","デフォルト値\n+HWID","BootRom","×","MBR内のSeed","NANDファーム","×","-","-","NANDドライバ","NANDドライバ FATFS暗号","アプリ管理画面","非公開"]
[]
[]
[null,"アプリがセーブデータに本体固有情報を絡めた暗号を使用することはガイドラインで禁止。"]